**Talking Pocket Alarm Silver Watch**

**(ES7105)**

**Instructions**

**Setting it up**

Your watch has 4 buttons on the edge of the case and a winding crown in the centre of the right hand edge. This crown should be pulled out to set the hands of the analogue display then pushed back in.

**How it works**

The top right button causes the time to be spoken.

The top left button selects the mode, either 'TIME' for normal running, 'SET ALARM' or 'SET TIME'. In the setting modes the lower left button alters the hours and the lower right alters the minutes.

In normal 'TIME' mode the lower left button is used to select between the cockerel, cuckoo or tone alarms or to turn the alarm off. The lower right button is used to select the hourly chime on or off.

To stop the alarm sounding press the top right button.

Please note that the analogue display is not connected to the speech system. This means that, if you wish, you may have one time being displayed and a different time being spoken.

Your watch uses 1 x CR-2016 Lithium and 1 x SR-626 Silver Oxide battery.