# Sensa Cup Level Indicator ES7119

# Product Instructions

# General description

Designed for single handed operation the SENSA is simply hung on the rim of the cup, mug or glass. It automatically adjusts itself for different types and sizes of container. Pour in the milk and a tone sounds for several seconds when the level reaches 1.3cm from the bottom.

# Instructions

Before using the "Sensa" make sure that the raised portion on the top is fully depressed with your finger.

Press the Sensa down on to the rim of the empty glass, cup, mug etc. with the probe inside, until the probe reaches the bottom of the container. The small area on the top will then rise by the appropriate amount to adjust to the height of the vessel being used.

Proceed to add the first amount of liquid to the vessel, i.e. milk, gin etc. When you hear the tone cease pouring. The first tone will stop after several seconds. Top up with the required liquid until the tone is heard again. Cease pouring. This second tone will continue until the Sensa is removed from the liquid.

After use, wipe the probe but DO NOT IMMERSE THE SENSA IN WATER.